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Abstract
Municipal solid wastes (MSW) collected from Padang Siding Landfill, Perlis were segregated and characterized in the laboratory. The main components of MSW found are paper, plastic, glass and large proportion of organic waste. Moisture content was measured for all the components. Paper and yard wastes recorded the highest percentage of 26.7% and 28.8%, respectively.  Thermogravimetric analysis (TGA) shows that the thermal degradation of MSW samples ranged from 200 oC to 800 oC, indicating fast decomposition occurred at 370 oC, 430 oC and 700 oC.  Traditional method shows a lower error compared to the physical method in calculating the calorific values (CV) for MSW. Bio-oil production via fast pyrolysis route gave higher liquid yield of ~35% with high oxygen content of ~49 – 53%. Heavy oil recovered from hydrous pyrolysis experiments gave low yield of ~7 – 13%, however with low oxygen content of ~11 – 18%. 

Keywords: Municipal solid waste, thermogravimetric analysis, calorific value, pyrolysis, hydrous pyrolysis

Abstrak
Sisa pepejal perbandaran (SPP) dikumpulkan dari tapak pelupusan Padang Siding, Perlis. Bahan buangan ini diasingkan dan dikategorikan di dalam makmal. Komponen utama MSW yang ditemui adalah kertas, plastik, kaca dan sebahagian besar sisa organik. Kandungan kelembapan diukur untuk semua komponen di mana kertas dan sisa dari laman telah mencatatkan peratus tertinggi sebanyak 26.7% dan 28.8% masing-masing. Analisis termogravimetrik menunjukkan degradasi terma sampel MSW adalah antara 200 oC hingga 800 oC, menunjukkan penguraian cepat berlaku pada 370 oC, 430 oC dan 700 oC. Kaedah tradisional menunjukkan ralat yang lebih rendah berbanding dengan kaedah fizikal dalam mengira nilai kalorifik  untuk SPP. Pengeluaran bio-minyak melalui laluan pirolisis pantas memberikan hasil cecair yang lebih tinggi  ~35% dengan kandungan oksigen yang tinggi ~ 49 – 53%. Minyak berat diperoleh daripada eksperimen pirolisis berair memberikan hasil yang rendah ~ 7 – 13%, walau bagaimanapun dengan kandungan oksigen yang rendah ~ 11 – 18%.

Kata kunci: Sisa pepejal perbandaran, analisa termogravimetrik, nilai kalorifik, pirolisis, pirolisis berair
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