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Abstract
Bisphenol A (BPA) is an industrial chemical applied in making polycarbonate and epoxy resin that commonly used as food containers, beverage cans and baby bottles. BPA could be discharged into the environment from industrial waste and sewage treatment plant which then causing adverse effects to aquatic organism and consumers. Micro-solid phase extraction (µ-SPE) using C18-impregnated cellulose triacetate (C18-CTA) composite film as the adsorbent films coupled with high performance liquid chromatography–fluorescence detection (HPLC-FD) has been developed for the determination of BPA in environmental water and soft drink samples. Under the optimum extraction conditions, the method showed excellent linearity in the range of 0.1 to 500 ppb with correlation coefficient, r = 0.992. This method provided ultra-trace detection limit of 0.004 ppb, trace quantification limit of 0.01 ppb and acceptable relative recovery average in the range of 80.9 to 102.6% with relative standard deviation ≤ 9.7%. The proposed microextraction method is simple, rapid and eco-friendly as it consumes less amount of non-hazardous organic solvent.
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Abstrak
Bisfenol A (BPA) ialah suatu bahan kimia industri yang digunakan dalam pembuatan polikarbonat dan resin epoksi yang biasa digunakan sebagai bekas makanan, tin minuman dan botol bayi. BPA boleh dilepaskan ke dalam alam sekitar daripada sisa industri dan loji rawatan kumbahan yang kemudiannya menyebabkan kesan buruk kepada organisma akuatik dan pengguna. Pengekstrakan mikro fasa pepejal (µ-SPE) menggunakan filem komposit selulosa triasetat berimpregnasi C18 (C18-CTA) sebagai filem penjerap berpasangan kromatografi cecair prestasi tinggi-pengesanan pendarfluor (HPLC-FD) telah dibangunkan untuk penentuan BPA dalam sampel air alam sekitar dan minuman ringan. Di bawah keadaan pengekstrakan optimum, kaedah ini menunjukkan kelinearan yang cemerlang daripada kepekatan 0.1 hingga 500 ppb dengan pekali korelasi, r = 0.992. Kaedah ini memberi had pengesanan ultra rendah iaitu 0.004 ppb, had kuantifikasi rendah iaitu 0.01 ppb dan purata pemulihan relatif yang boleh diterima dalam lingkungan 80.9 hingga 102.6% dengan sisihan piawai relatif ≤ 9.7%. Pengekstrakan mikro yang dicadangkan adalah bermanfaat daripada segi operasi mudah, cepat dan mesra alam kerana ia menggunakan sedikit pelarut organik yang tidak berbahaya.
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