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Abstract
This study aims to develop a small size of TNF using an electrospinning process. TNF is applied in direct methanol fuel cell (DMFC) as a catalyst, catalyst support and a filler in the membrane. This study involves determining the parameters that affect the electrospinning process, particularly in terms of the distance between the needle tip and collector towards the size of TNF crystalline. The production of TNF involves an electrospinning process, followed by a stabilization and calcination process. Fourier Transformation Infrared (FTIR) analysis was carried out to analyse the purity of the samples, while X-ray diffractometer (XRD) analysis was carried out to determine the size of crystalline. The result demonstrates that the longer the distance between the needle and collector, the smaller the size of the TNF produced. A smaller sized crystalline offers a significant impact on catalytic reaction and overall performance of DMFC. 
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Abstrak
Objektif utama kajian ini ialah membangunkan TNF bersaiz kecil untuk proses elektroputaran. Penggunaan TNF dalam sel bahan api metanol langsung (DMFC) adalah sebagai mangkin, sokongan mangkin dan pengisi di dalam membran. Kajian ini dijalankan untuk menentukan parameter yang dapat menjejaskan proses elektroputaran, iaitu jarak antara hujung jarum dan pengumpul, terhadap saiz habluran TNF. Penghasilan TNF melibatkan proses elektroputaran, diikuti dengan penstabilan dan kalsinasi. Analisis infra merah transformasi Fourier (FTIR) dijalankan untuk menganalisa ketulenan sampel, sementara analisis pembelauan sinar-X (XRD) untuk menentukan saiz habluran. Keputusan ujikaji menunjukkan semakin jauh jarak antara hujung jarum dan pengumpul, semakin kecil saiz TNF yang diperolehi. Pengurangan saiz habluran memberikan kesan yang besar kepada tindak balas pemangkinan dan prestasi keseluruhan DMFC.
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