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Abstract
Multi walled carbon nanotubes (MWCNT) hold the increasing interest in many different fields. To employ MWCNT as an effective reinforcement in order to enhance the thermal conductivity of polylactic acid (PLA) modified with liquid natural rubber (LNR), proper dispersion and appropriate interfacial adhesion between MWCNT and PLA/LNR have to be guaranteed. This paper used ultrasonic technique as the method to help to improve the dispersion of MWCNT in PLA/LNR matrix. The result shown that the sample with 3.5 wt.% of MWCNT provided higher thermal conductivity which is believe to be the optimum loading due to better dispersion of MWCNT in PLA/LNR matrix. The 4 wt.% of MWCNT shows decreasing of thermal conductivity due to the presence of agglomeration of MWCNT. The results confirmed by Scanning Electron Microscopy (SEM) micrograph. Fourier Transform Infrared (FTIR) spectra shown that there were no chemical changes happen.
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Abstrak
Tiub karbon berbilang dinding (MWCNT) telah menarik minat dalam pelbagai bidang yang berbeza. Bagi memastikan MWCNT dapat digunakan secara berkesan sebagai agen pengukuh dalam peningkatan kekonduksian terma polilaktik asid (PLA)/ cecair getah asli (LNR) nanokomposit, serakan dan lekatan antara muka yang sempurna dan baik di antara MWCNT dan PLA/LNR adalah di antara aspek yang perlu diberi perhatian. Di dalam kertas ini, teknik ultrasonik telah digunakan bagi memastikan membantu penyerakan MWCNT di dalam PLA/LNR matrik. Keputusan menunjukkan sampel yang mengandungi 3.5 wt% MWCNT menghasilkan kekonduksian terma yang tertinggi dengan pencapaian nilai kandungan optima disebabkan oleh serakan yang baik di dalam PLA/LNR matrik. Pada kandungan MWCNT 4 wt%, kekonduksian terma menunjukkan penurunan disebabkan oleh gumpalan MWCNT. Keputusan disahkan oleh Imbasan Elektron Microskopi (SEM) mikrograf. Spektra Fourier Transform Inframerah Spektroskopi (FTIR) pula menunjukkan tiada perubahan kimia yang berlaku.
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